------------------------------------------------------------------------------
WIRESMON-X.EXE (WIRES-X Remote Monitor application) ver.2.000
                        Copyright(c) YAESU MUSEN CO., LTD.
------------------------------------------------------------------------------


((( Getting started )))

WIRESMON-X.EXE is a application that allows you to monitor and control your
WIRES-X Node from a remote location, using an Internet connection. 
( WIRES = Wide-Coverage Internet Repeater Enhancement System )

With WIRESMON-X.EXE, you can perform the following tasks:

* Monitor of the audio passing through your Node;
* Display of Node to which you are connected;
* ON-AIR LOCK control (transmission lockout and TX shutdown); and
* Restart of WIRES-X application
* Web monitor function




((( System Requirements )))

In order to use this application, a personal computer (PC) with the following
operating system is required.

1.Operating system (OS)
Microsoft Windows 11

2.CPU
Processor Clock Frequency: 1.0GHz or faster(recommended).

3.RAM (system memory)
4GB or more(recommended).

4.Strage
The capacity of the HDD/SSD must be more than sufficient to satisfy the operating
system requirements.

5.Diplay resolution
1024 * 768 or higher (16-bit high color or higher)

6.LAN port
100BASE-TX or higher(recommended)

7.Internet connection
* 8Mbps or faster (high-speed connection recommended)
* IPv4 address Internet line.(Global IP addresses and port routing are not required.)
* Firewall software settings are required.




((( Installation / Un-installation )))

1.Installation
The PC hardware requirements for use of this application are identical to those
for regular WIRES-X operation.

The WIRESMON-X application must, however, be installed in a different
computer from the one actually running your monitoring Node.

* The IPv4 address with Internet access is required.
  (Global IP addresses and port routing are not required.)

* Configure your PC's firewall software to allow communication.

* When using the web monitor function, it is necessary to open the TCP port
  in the node PC and external firewall settings.

* To utilize this application, the DTMF ID and Serial number for the associated
  HRI-200 Interface Box will be required. 
  Password security is available, as well.

* This application can control WIRES-X IPv6 compatible ver.
  (cannot control ver1.570 or earlier)

* From the download site, download the wiresmon-x2000en.zip file and store it
  in the folder of your choosing.

* All elements required for operation are included in the downloaded zip file,
  so after you unzip the application into the desired folder, you will be ready
  for operation.


The files installed from the zip file include:

* WIRESMON-X.EXE : This is the main executable application file.
* DlgComFuncs.dll : DLL application file for WIRESMON-X.exe.
* UdpComFuncs.dll : DLL application file for WIRESMON-X.exe.
* WIRESMON-X.chm : WIRES-X remote monitor online help
* WIRESMON-X.txt : WIRES-X remote monitor text document

The following setting information file(.ini) are generated by a standard
document folder ( \Documents\WIRESXA\ ).

* WIRESMON-X.INI : This is the remote configuration file, used at startup.


2.Un-installation
To un-install the application, just delete the above installed files.




((( Operation )))


1.Start WIRESMON-X application

(1)PC Firewall setting
Firewall software is installed as a standard feature in windows PC.
When the WIRESMON-X application is started up for the first time, a message
regarding communication block is displayed by the firewall software.
Configure the system to permit communications to be carried out.


(2)Access Setting
When the application starts up, you need to input the information listed below,
so as to allow your application to communicate with your node.

Please input the following information.

DTMF ID   : DTMF ID number of your Node.
Serial No : Serial number of your Node's HRI-200 I/F Box.
Password  : Remote control's Password which you must have set on your Node
            computer.
Save Password : When you have finished entering it, so as to allow your
                computer to remember it.

* Prior to attempting Remote Control operation, you must modify the settings
  your node's WIRES-X application to set Remote Control function to ON.
  ([File]-[Settings]-[Property]-[General settings])


(3)Connect
When you click on "Connect", your remote monitor application and the monitoring
WIRES-X node will be connected, via the Internet.

If not connected, the following messages may be shown.

"Server or ID Not Found"
Be sure the DTMF ID and Serial No. all match the registration.
Also, when the communication is not established because of the FireWall
(no port is assigned).

"Password Unmatch"
The password which is programmed on the WiRES-II terminal does not match the
password input.


(4)Disconnect
To disconnect and end remote monitoring, just click on "Disconnect".




--------------------------------------------------------------------------------
2.WIRES-X Monitor

The state of the WIRES-X application is displayed as follows.

User ID  : User ID of monitoring WIRES-X Node is displayed here.
CallSign : CallSign of monitoring WIRES-X Node is displayed here.


[IDLE]&[NET]
This area displays the operating status of monitoring Node.
  
The display switches between Analog/Digital/GM depending on the transceiver
setting and operation style setting.

IDLE is displayed (in gray) if the station is not connected to other Node/Room.
NET is displayed (in green) if the station is being connected to other
Node/Room.


[ON-AIR]&[ON-AIR LOCK]
Display the transmission status of monitoring Node.
Upper:Voice CH / Lower:Preset search CH
ON-AIR(Gray)  : No Transmitting
ON-AIR(Green) : Transmitting
ON-AIR LOCK   : ON-AIR LOCK(Transmission is prohibited) status


[LOCAL]&[INTERNET]
Display the reception status of monitoring Node.
Upper:Voice CH / Lower:Preset search CH
LOCAL(Gray)  : No signal
LOCAL(Blue)  : Receiving signal (SQL code differs from the setting)
LOCAL(Green) : Receiving signal (SQL code matching/Not voice relaying)
INTERNET     : Relaying voice signal to connecting Node/Room.


[HRI-200]
Display the connection status between the WIRES application (PC) and HRI-200.
"RADIO 1" and "RADIO2" is displayed when detected the HRI-200 mode transceiver.
If PC is displaying HRI-200(Red) icon, PC is not detected the HRI-200.


[Connecting Node/Room ID]
Display the User ID of WIRES Node/Room that are connected.


--------------------------------------------------------------------------------
3.WIRES-X Control

(1)SOUND Monitor
This button is switch of the voice sound monitoring function.
When you click on this button, you will be able to monitor both sides of
the audio being passed through your Node. If you use this function,
the monitoring node must be in the "NET"(connecting) state.

SOUND Monitor(BLUE) : Monitoring
SOUND Monitor(Gray) : Monitor OFF



(2)ON-AIR ACTIVE / LOCK
This button is switch of the ON-AIR LOCK function.
When you click on this button, you can control transmission status of
your monitoring Node.

ON-AIR ACTIVE : Normal Operation
ON-AIR LOCK   : ON-AIR LOCK(Transmission is prohibited) status)



(3)App Quit
By this button, you can perform the exit operation that is equal to
[File]-[Exit] command.

When Auto Start function of YMLAN.exe becomes ON, you can perform restart
the WIRES-X application in remoteness.



(4)Web monitor function
When you pushed the [Web monitor] button, you can display information of
a state and the setting of monitoring WIRES-X node using web browser.

(4-1)The setting of the remote monitor application is as follows.

* Web port (TCP port number)
Please input the TCP Port number that matches the monitoring WIRES-X Node's
setting.

* Web Monitor button
When you pushed this button, you can display information of monitoring node
using web browser.


(4-2)The setting of the monitoring WIRES-X node is as follows.

* TCP Port routing(opening) setting to the Router(NAPT etc.) and the firewall
  setting of WIRES-X application.

* Setup of the WebServer plugin(WiresWeb.dll).
  (For details, see the WIRES-X Instruction Manual.)



(5)Sound Volume Control
By this function, you can adjust the audio level(volume) of remote monitor
application.

* You can adjust the volume of the remote monitoring PC, but cannot adjust
  the volume of monitoring Node's PC.

* This volume control funtion links the "WIRES Monitor application Volume
  (Applications)" in the Volume Mixer screen of the OS.
  Please adjust the "Speaker volume(Device/System)" volume when appropriate volume
  does not have it.



(6)[Close] button
Click here to Exit this window.




